Planar R140 Vector Reflectometer (Analyzer)
Software Installation Guide


I. CD Contents

1. 
1. Setup_PlanarR140_vX.X.exe Installer File
2. Setup_PlanarR140_vX.X_DEMO.exe Installer File
3. Setup_PlanarR140x2_vX.X.exe Installer File
2. Driver in the Driver Folder
3. README.TXT File
4. Documentation in the Doc Folder


II. PC Minimum System Requirements

1. OS WINDOWS 2000/XP/VISTA/7
2. 1 GHz Processor
3. 512 MB RAM
4. USB 2.0
5. 800x600 VGA Display


III. Software Installation

The software installation procedure includes the USB driver installation and the program
installation. The USB driver is installed in the standard Windows dialog when the Analyzer
is connected to the PC for first time. The rest of the software is installed by
the Setup_PlanarR140x2_vX.X.exe installer file, where X.XX is the number of the software version.


IV. USB Driver Installation

1. Connect the Analyzer to your PC via the supplied USB cable. It is allowed to connect
the USB cable to the running PC.
2. Turn on and boot the PC, if it is off.
3. When you connect the Analyzer to the PC for the first time, Windows will automatically
detect the new USB device and will open the USB driver installation dialog (Windows 2000/XP/VISTA).
In Windows 7, open the USB driver installation dialog as follows:
Start > Control Panel > Device Manager.
Make the right mouse click on the 'Unknown Device' line and select 'Update Drivers'.
4. In the USB driver installation dialog, click on 'Browse' and specify the path to
the driver files, which are contained in the \DRIVER folder.
5. When the driver is installed, the new USB device (PLANAR R140 Vector Reflectometer) will appear
in the system.


V. Program Installation

To install the program, run the Setup_PlanarR140_vX.X.exe, Setup_PlanarR140_vX.X_DEMO.exe and/or Setup_PlanarR140x2_vX.X.exe installer file from the CD.
Follow the instructions of the installation wizard until the program is installed.
If you install the program in demo mode, installation of the USB driver is not required.
